<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<library>
<packages>
<package name="TSSOP20-08THIN">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="SSOP16">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt; SSOP 16 (5.3mm x 6.2mm)&lt;p&gt;
Source: www.austriamicrosystems.com .. AS5040DataSheetRev12.pdf</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;</description>
</package>
<package name="VL53L0X">
</package>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="TO-92-AMMO">
<description>&lt;h3&gt;TO-92 3-Pin PTH AMMO package&lt;/h3&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 3&lt;/li&gt;
&lt;li&gt;Dimensions:  3.68 x 4.83 x 4.83 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;DS18B20&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="LGA-24-3.5X3">
<description>&lt;h3&gt;24-pin LGA (3.5 x 3 mm)&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/assets/learn_tutorials/3/7/3/LSM9DS1_Datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 24&lt;/li&gt;
&lt;li&gt;Area: 3.5 x 3.0 mm&lt;/li&gt;
&lt;li&gt;Pitch: 0.43 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;LSM9DS1&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
<symbols>
<symbol name="AS5304-6">
<pin name="VSS"/>
<pin name="A"/>
<pin name="VDDP"/>
<pin name="B"/>
<pin name="TEST1"/>
<pin name="AO"/>
<pin name="VDD"/>
<pin name="INDEX"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="TEST2"/>
<pin name="TEST3"/>
<pin name="TEST4"/>
<pin name="TEST_GND"/>
<pin name="VDDA"/>
<pin name="TEST5"/>
<pin name="TEST6"/>
<pin name="TEST7"/>
<pin name="ZPZ"/>
</symbol>
<symbol name="AS5040">
<pin name="MAGINC" direction="hiz"/>
<pin name="MAGDEC" direction="hiz"/>
<pin name="A_LSB_U" direction="out"/>
<pin name="B_DIR_V" direction="out"/>
<pin name="COIL" direction="nc"/>
<pin name="INDEX_W" direction="out"/>
<pin name="VSS" direction="pas"/>
<pin name="PROG" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="CLK" direction="in"/>
<pin name="CSN" direction="in"/>
<pin name="PWN" direction="pas"/>
<pin name="T_B_0" direction="nc"/>
<pin name="T_B_1" direction="nc"/>
<pin name="VDD3V3" direction="pas"/>
<pin name="VDD5V" direction="pas"/>
</symbol>
<symbol name="AS5047">
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="CLK"/>
<pin name="CSN"/>
<pin name="TEST"/>
<pin name="A"/>
<pin name="B"/>
<pin name="I"/>
<pin name="GND"/>
<pin name="VDD3V"/>
<pin name="VDD"/>
<pin name="U"/>
<pin name="V"/>
<pin name="W"/>
</symbol>
<symbol name="VL53L0X">
<pin name="AVDD"/>
<pin name="AVDDVCSEL"/>
<pin name="DNC"/>
<pin name="GND"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="XSHUT"/>
<pin name="AVSSVCSEL"/>
<pin name="GPIO1"/>
</symbol>
<symbol name="AEAT-6600">
<pin name="A"/>
<pin name="B"/>
<pin name="I"/>
<pin name="MAG_HI"/>
<pin name="MAG_LO"/>
<pin name="GND"/>
<pin name="ALIGN"/>
<pin name="PWM"/>
<pin name="VDD"/>
<pin name="VDD_F"/>
<pin name="PWRDOWN"/>
<pin name="VPP"/>
<pin name="PROG"/>
<pin name="NCS"/>
<pin name="CLK"/>
<pin name="DO/DI"/>
</symbol>
<symbol name="HALL-SWITCH-S5712">
<pin name="GND"/>
<pin name="VDD"/>
<pin name="OUT"/>
</symbol>
<symbol name="HALL-DRV5053">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="LSM9DS1">
<description>&lt;h3&gt;ST Microelectronics LSM9DS1 9DOF IMU - Accelerometer, Gyroscope &amp; Magnetometer&lt;/h3&gt;
&lt;p&gt;The LSM9DS1 is a versatile, motion-sensing system-in-a-chip. It houses a 3-axis accelerometer, 3-axis gyroscope, and 3-axis magnetometer – nine degrees of freedom (9DOF) in a single IC! The LSM9DS1 is equipped with a digital interface, but even that is flexible: it supports both I2C and SPI, so you’ll be hard-pressed to find a microcontroller it doesn’t work with.&lt;/p&gt;</description>
<pin name="GND"/>
<pin name="C1"/>
<pin name="CAP"/>
<pin name="DEN_A/G"/>
<pin name="INT_M"/>
<pin name="DRDY_M"/>
<pin name="INT1_A/G"/>
<pin name="INT2_A/G"/>
<pin name="VDD"/>
<pin name="VDDIO"/>
<pin name="CS_M"/>
<pin name="CS_A/G"/>
<pin name="SCL/SPC"/>
<pin name="SDO_M"/>
<pin name="SDO_A/G"/>
<pin name="SDA/SDI/SDO"/>
<pin name="RSVD"/>
</symbol>
<symbol name="RTD-NI1000SOT">
<pin name="TERM1"/>
<pin name="TERM2"/>
<pin name="SENSE"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AS5304-6">
<gates>
<gate name="G$1" symbol="AS5304-6"/>
</gates>
<devices>
<device name="" package="TSSOP20-08THIN">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="AO" pad="6"/>
<connect gate="G$1" pin="B" pad="4"/>
<connect gate="G$1" pin="INDEX" pad="8"/>
<connect gate="G$1" pin="NC1" pad="9"/>
<connect gate="G$1" pin="NC2" pad="10"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="TEST1" pad="5"/>
<connect gate="G$1" pin="TEST2" pad="12"/>
<connect gate="G$1" pin="TEST3" pad="13"/>
<connect gate="G$1" pin="TEST4" pad="14"/>
<connect gate="G$1" pin="TEST5" pad="17"/>
<connect gate="G$1" pin="TEST6" pad="18"/>
<connect gate="G$1" pin="TEST7" pad="19"/>
<connect gate="G$1" pin="TEST_GND" pad="15"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="16"/>
<connect gate="G$1" pin="VDDP" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="ZPZ" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AS5040" prefix="IC">
<description>&lt;b&gt;10-BIT PROGRAMMABLE MAGNETIC ROTARY ENCODER&lt;/b&gt;&lt;p&gt;
Source: www.austriamicrosystems.com .. AS5040DataSheetRev12.pdf</description>
<gates>
<gate name="G$1" symbol="AS5040"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="G$1" pin="A_LSB_U" pad="3"/>
<connect gate="G$1" pin="B_DIR_V" pad="4"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="COIL" pad="5"/>
<connect gate="G$1" pin="CSN" pad="11"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="INDEX_W" pad="6"/>
<connect gate="G$1" pin="MAGDEC" pad="2"/>
<connect gate="G$1" pin="MAGINC" pad="1"/>
<connect gate="G$1" pin="PROG" pad="8"/>
<connect gate="G$1" pin="PWN" pad="12"/>
<connect gate="G$1" pin="T_B_0" pad="13"/>
<connect gate="G$1" pin="T_B_1" pad="14"/>
<connect gate="G$1" pin="VDD3V3" pad="15"/>
<connect gate="G$1" pin="VDD5V" pad="16"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AS5040ASSU"/>
<attribute name="OC_FARNELL" value="1630800"/>
<attribute name="OC_NEWARK" value="59P4059"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AS5047">
<gates>
<gate name="G$1" symbol="AS5047"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CSN" pad="1"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="I" pad="14"/>
<connect gate="G$1" pin="MISO" pad="3"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="TEST" pad="5"/>
<connect gate="G$1" pin="U" pad="10"/>
<connect gate="G$1" pin="V" pad="9"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD3V" pad="12"/>
<connect gate="G$1" pin="W" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VL53L0X" prefix="U">
<description>VL53L0X distance sensor</description>
<gates>
<gate name="G$1" symbol="VL53L0X"/>
</gates>
<devices>
<device name="" package="VL53L0X">
<connects>
<connect gate="G$1" pin="AVDD" pad="11"/>
<connect gate="G$1" pin="AVDDVCSEL" pad="1"/>
<connect gate="G$1" pin="AVSSVCSEL" pad="2"/>
<connect gate="G$1" pin="DNC" pad="8"/>
<connect gate="G$1" pin="GND" pad="3 4 6 12"/>
<connect gate="G$1" pin="GPIO1" pad="7"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="XSHUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AEAT-6600" prefix="U">
<gates>
<gate name="G$1" symbol="AEAT-6600"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="ALIGN" pad="7"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="CLK" pad="15"/>
<connect gate="G$1" pin="DO/DI" pad="16"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="I" pad="3"/>
<connect gate="G$1" pin="MAG_HI" pad="4"/>
<connect gate="G$1" pin="MAG_LO" pad="5"/>
<connect gate="G$1" pin="NCS" pad="14"/>
<connect gate="G$1" pin="PROG" pad="13"/>
<connect gate="G$1" pin="PWM" pad="8"/>
<connect gate="G$1" pin="PWRDOWN" pad="11"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VDD_F" pad="10"/>
<connect gate="G$1" pin="VPP" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HALL-SWITCH-S5712" prefix="U">
<gates>
<gate name="G$1" symbol="HALL-SWITCH-S5712"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HALL-DRV5053" prefix="U">
<gates>
<gate name="G$1" symbol="HALL-DRV5053"/>
</gates>
<devices>
<device name="" package="TO-92-AMMO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LSM9DS1" prefix="U">
<description>&lt;h3&gt;ST Microelectronics LSM9DS1 9DOF IMU - Accelerometer, Gyroscope &amp; Magnetometer&lt;/h3&gt;
&lt;p&gt;The LSM9DS1 is a versatile, motion-sensing system-in-a-chip. It houses a 3-axis accelerometer, 3-axis gyroscope, and 3-axis magnetometer – nine degrees of freedom (9DOF) in a single IC! The LSM9DS1 is equipped with a digital interface, but even that is flexible: it supports both I2C and SPI, so you’ll be hard-pressed to find a microcontroller it doesn’t work with.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/assets/learn_tutorials/3/7/3/LSM9DS1_Datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13284"&gt;SparkFun 9 Degrees of Freedom IMU Breakout - LSM9DS1&lt;/a&gt; (SEN-13284)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13629"&gt;SparkFun Photon IMU Shield&lt;/a&gt; (DEV-13629)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="LSM9DS1"/>
</gates>
<devices>
<device name="" package="LGA-24-3.5X3">
<connects>
<connect gate="G$1" pin="C1" pad="24"/>
<connect gate="G$1" pin="CAP" pad="21"/>
<connect gate="G$1" pin="CS_A/G" pad="7"/>
<connect gate="G$1" pin="CS_M" pad="8"/>
<connect gate="G$1" pin="DEN_A/G" pad="13"/>
<connect gate="G$1" pin="DRDY_M" pad="9"/>
<connect gate="G$1" pin="GND" pad="19 20"/>
<connect gate="G$1" pin="INT1_A/G" pad="11"/>
<connect gate="G$1" pin="INT2_A/G" pad="12"/>
<connect gate="G$1" pin="INT_M" pad="10"/>
<connect gate="G$1" pin="RSVD" pad="14 15 16 17 18"/>
<connect gate="G$1" pin="SCL/SPC" pad="2"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="4"/>
<connect gate="G$1" pin="SDO_A/G" pad="5"/>
<connect gate="G$1" pin="SDO_M" pad="6"/>
<connect gate="G$1" pin="VDD" pad="22 23"/>
<connect gate="G$1" pin="VDDIO" pad="1 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12536"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTD-NI1000SOT" prefix="U">
<gates>
<gate name="G$1" symbol="RTD-NI1000SOT"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="SENSE" pad="3"/>
<connect gate="G$1" pin="TERM1" pad="1"/>
<connect gate="G$1" pin="TERM2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
