<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<library>
<packages>
<package name="LQFP48">
<description>&lt;b&gt;48-pin plastic LQFP (FPT-48P-M26)&lt;/b&gt;&lt;p&gt;
www.fma.fujitsu.com/pdf/e713717.pdf</description>
</package>
<package name="TQFP100-14X14">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt; 14x14 mm&lt;p&gt;</description>
</package>
<package name="QFN-64-9X9MM">
<description>&lt;h3&gt;64-pin QFN 9x9mm, 0.5mm pitch&lt;/h3&gt;
&lt;p&gt;Package used by ATmega128RFA1&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.atmel.com/Images/Atmel-8266-MCU_Wireless-ATmega128RFA1_Datasheet.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TC2030-MCP">
<description>&lt;b&gt;TAG-CONNECT ICSP Connector&lt;/b&gt; - Legged version&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="http://www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;
&lt;p&gt;
Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.
&lt;p&gt;
&lt;b&gt;NOTE:&lt;/b&gt; Eagle's default spacing for drill holes does not leave sufficent room for routing traces for this footprint and should be adjusted. &lt;br&gt;
This setting can be found in the board layout editor under the Edit menu.  Select "Design Rules" and then the Distance tab.  8 mils for Drill/Hole works well.
&lt;br&gt;
&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;
©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
</package>
<package name="TC2030-MCP-NL">
<description>&lt;B&gt;TAG-CONNECT ICSP Connector&lt;/B&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.&lt;BR&gt;

&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
</package>
<package name="TC2030-MCP-NL-CP">
<description>&lt;B&gt;TAG-CONNECT ICSP Connector&lt;/B&gt;&lt;I&gt;- with optional copper pads for steel alignment pins&lt;/I&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="http://www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.
&lt;p&gt;
&lt;b&gt;NOTE:&lt;/b&gt; Eagle's default spacing for drill holes does not leave sufficent room for routing traces for this footprint and should be adjusted. &lt;br&gt;
This setting can be found in the board layout editor under the Edit menu.  Select "Design Rules" and then the Distance tab.  8 mils for Drill/Hole works well.
&lt;br&gt;
&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Note:&lt;/B&gt; Suitable Receptacle pins are 0295-0-15-xx-06-xx-10-0 series from &lt;a href="www.mill-max.com"&gt;Mill-Max&lt;/a&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
</package>
</packages>
<symbols>
<symbol name="ATSAM4N8A">
<pin name="ADVREFP"/>
<pin name="GND_1"/>
<pin name="PB0/AD4"/>
<pin name="PB1/AD5"/>
<pin name="PB2/AD6"/>
<pin name="PB3/AD7"/>
<pin name="VDDIN"/>
<pin name="VDDOUT"/>
<pin name="PA17/PGMD5/AD0"/>
<pin name="PA18/PGMD6/AD1"/>
<pin name="PA19/PGMD7/AD2"/>
<pin name="PA20/AD3"/>
<pin name="VDDIO_1"/>
<pin name="PA16/PGMD4"/>
<pin name="PA15/PGMD3"/>
<pin name="PA14/PGMD2"/>
<pin name="PA13/PGMD1"/>
<pin name="VDDCORE_1"/>
<pin name="PA12/PGMD0"/>
<pin name="PA11/PGMM3"/>
<pin name="PA10/PGMM2"/>
<pin name="PA9/PGMM1"/>
<pin name="PA8/XOUT32/PGMM0"/>
<pin name="PA7/XIN32/PGMNVALID"/>
<pin name="TDI/PB4"/>
<pin name="PA6/PGMNOE"/>
<pin name="PA5/PGMRDY"/>
<pin name="PA5/PGMNCMD"/>
<pin name="NRST"/>
<pin name="TST"/>
<pin name="PA3"/>
<pin name="PA2/PGMEN2"/>
<pin name="VDDIO_2"/>
<pin name="GND_2"/>
<pin name="PA1/PGMEN1"/>
<pin name="PA0/PGMEN0"/>
<pin name="TDO/TRACESWO/PB5"/>
<pin name="JTAGSEL"/>
<pin name="TMS/SWDIO/PB6"/>
<pin name="TCK/SWCLK/PB7"/>
<pin name="VDDCORE_2"/>
<pin name="ERASE/PB12"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="XOUT/PB8"/>
<pin name="XIN/P/PB9/GMCK"/>
<pin name="VDDIO_3"/>
<pin name="VDDPLL"/>
</symbol>
<symbol name="ATSAMS70N">
<pin name="PA0/I2SC0_MCK"/>
<pin name="PA1/I2SC0_CK"/>
<pin name="PA2"/>
<pin name="PA3/TWD0"/>
<pin name="PA4/UTXD1/TWCK0"/>
<pin name="PA5/URXD1"/>
<pin name="PA7/XIN32"/>
<pin name="PA8/XOUT32"/>
<pin name="PA9/URXD0"/>
<pin name="PA10/UTXD0"/>
<pin name="PA11/PWMC0_PWMH0"/>
<pin name="PA12/PWMC0_PWMH1"/>
<pin name="PA13/PWMC0_PWMH2"/>
<pin name="PA14/WMC0_PWMH3"/>
<pin name="PA15/PWMC0_PWML3"/>
<pin name="PA16/PWMC0_PWML2"/>
<pin name="PA17/AFE0_AD6"/>
<pin name="PA18/AFE0_AD7"/>
<pin name="PA19/PWMC0_PWML0/AFE0_AD8"/>
<pin name="PA20/PWMC0_PWML1/AFE0_AD9"/>
<pin name="PA21/AFE0_AD1"/>
<pin name="PA22"/>
<pin name="PA23"/>
<pin name="PA24"/>
<pin name="PA25"/>
<pin name="PA26"/>
<pin name="PA27"/>
<pin name="PA28"/>
<pin name="PA30"/>
<pin name="PA31/SPI0_NPCS1"/>
<pin name="PB0/RXD0"/>
<pin name="PB1/TXD0"/>
<pin name="PB2/SPI0_NPCS0/CTS0"/>
<pin name="PB3/RTS0"/>
<pin name="PB4/TDI/TWD1"/>
<pin name="PB5/TDO/TWCK1"/>
<pin name="PB6/SWDIO/TMS"/>
<pin name="PB7/SWCLK/TCK"/>
<pin name="PB8/XOUT"/>
<pin name="PB9/XIN"/>
<pin name="PB12/ERASE"/>
<pin name="PB13/DAC0/SCK0"/>
<pin name="PD1/PWMC1_PWMH0"/>
<pin name="PD2/PWMC1_PWML1"/>
<pin name="PD3/PWMC1_PWMH1"/>
<pin name="PD4/PWMC1_PWML2"/>
<pin name="PD5/PWMC1_PWMH2"/>
<pin name="PD6/PWMC1_PWML3"/>
<pin name="PD7/PWMC1_PWMH3"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10/PWMC0_PWML0"/>
<pin name="PD11/PWMC0_PWMH0"/>
<pin name="PD12/SPI0_NPCS2"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PD16"/>
<pin name="PD17"/>
<pin name="PD18/URXD4"/>
<pin name="PD19/UTXD4"/>
<pin name="PD20/SPI0_MISO"/>
<pin name="PD21/SPI0_MOSI"/>
<pin name="PD22_SPI0_SPCK"/>
<pin name="PD24"/>
<pin name="PD25/URXD2"/>
<pin name="PD26/UTXD2"/>
<pin name="PD27/SPI0_NPCS3/TWD2"/>
<pin name="PD28/URXD3/TWCK2"/>
<pin name="PD30/UTXD3"/>
<pin name="PD31"/>
<pin name="PD0/DAC1/PWMC1_PWML0"/>
<pin name="VDDIO1"/>
<pin name="VDDIO2"/>
<pin name="VDDIO3"/>
<pin name="VDDIO4"/>
<pin name="JTAGSEL"/>
<pin name="TST"/>
<pin name="VREFP"/>
<pin name="NRST"/>
<pin name="VDDOUT"/>
<pin name="VDDIN"/>
<pin name="VREFN"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="VDDPLL"/>
<pin name="VDDUTMII"/>
<pin name="VDDUTMIC"/>
<pin name="VBG"/>
<pin name="GND6"/>
<pin name="GND5"/>
<pin name="VDDCORE1"/>
<pin name="VDDCORE2"/>
<pin name="VDDCORE3"/>
<pin name="VDDCORE4"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="VDDPLLUSB"/>
</symbol>
<symbol name="ATSAMD51">
<pin name="GND@5"/>
<pin name="GND@4"/>
<pin name="GND@3"/>
<pin name="GND@2"/>
<pin name="GND@1"/>
<pin name="VDDCORE"/>
<pin name="VDDANA"/>
<pin name="VDDIO@4"/>
<pin name="VDDIO@3"/>
<pin name="VDDIO@2"/>
<pin name="VDDIO@1"/>
<pin name="PA00/SER1-0/TC2-0"/>
<pin name="PA01/SER1-1/TC2-1"/>
<pin name="PA02/ADC0-1/DAC-0"/>
<pin name="PA03/ANAREF-VREFA/ADC0-1"/>
<pin name="PA04/ANAREF-VREFB/ADC0-4/SER0-0/TC0-0"/>
<pin name="PA05/ADC0-5/DAC-1/SER0-1/TC0-1"/>
<pin name="PA06/ANAREF-VREFC/ADC0-6/SER0-2/TC1-0"/>
<pin name="PA07/ADC0-7/SER0-3/TC1-1"/>
<pin name="PA08/ADC0-8/ADC1-2/SER0-0/SER2-1/TC0-0"/>
<pin name="PA09/ADC0-9/ADC1-3/SER0-1/SER2-0/TC0-1"/>
<pin name="PA10/ADC0-10/SER0-2/SER2-2/TC1-0"/>
<pin name="PA11/ADC0-11/SER0-3/SER2-3/TC1-1"/>
<pin name="PA12/SER2-0/SER4-1/TC2-0"/>
<pin name="PA13/SER2-1/SER4-0/TC2-1"/>
<pin name="PA14/SER2-2/SER4-2/TC3-0"/>
<pin name="PA15/SER2-3/SER4-3/TC3-1"/>
<pin name="PA16/SER1-0/SER3-1/TC2-0"/>
<pin name="PA17/SER1-1/SER3-0/TC2-1"/>
<pin name="PA18/SER1-2/SER3-2/TC3-0"/>
<pin name="PA19/SER1-3/SER3-3/TC3-1"/>
<pin name="PA20/SER5-2/SER3-2/TC7-0"/>
<pin name="PA21/SER5-3/SER3-3/TC7-1"/>
<pin name="PA22/SER3-0/SER5-1/TC4-0"/>
<pin name="PA23/SER3-1/SER5-0/TC4-1"/>
<pin name="PA24/SER3-2/SER5-2/TC5-0/USBDM"/>
<pin name="PA25/SER3-3/SER5-3/TC5-1/USBDP"/>
<pin name="PA27/GCLK-1"/>
<pin name="PA30/SER7-2/SER1-2/TC6-0/SWCLK"/>
<pin name="PA31/SER7-3/SER1-3/TC6-1"/>
<pin name="PB00/ADC0-12/SER5-2/TC7-0"/>
<pin name="PB01/ADC0-13/SER5-3/TC7-1"/>
<pin name="PB03/ADC0/SER5-1/TC6"/>
<pin name="PB04/ADC1-6"/>
<pin name="PB05/ADC1-7"/>
<pin name="PB06/ADC1-8"/>
<pin name="PB07/ADC1-9"/>
<pin name="PB08/ADC0-2/ADC1-9/SER4-0/TC4-0"/>
<pin name="PB09/ADC0-3/ADC1-1/SE4-1/TC4-1"/>
<pin name="PB10/SER4-2/TC5-0"/>
<pin name="PB11/SER4-3/TC5-1"/>
<pin name="PB12/SER4-0/TC4-0"/>
<pin name="PB13/SER4-1/TC4-1"/>
<pin name="PB14/SER4-2/TC5-0"/>
<pin name="PB15/SER4-3/TC5-1"/>
<pin name="PB16/SER5-0/TC6-0"/>
<pin name="PB17/SER5-1/TC6-1"/>
<pin name="PB22/SER1-2/SER5-2/TC7-0"/>
<pin name="PB23/SER1-3/SER5-3/TC7-1"/>
<pin name="PB30/SER7-0/SER5-1/TC0-0/SWDIO"/>
<pin name="RESETN"/>
<pin name="PB31/SER7-1/SER5-0/TC0-1"/>
<pin name="PB02/ADC0-14/SER5-0/TC6-0"/>
<pin name="VSW"/>
</symbol>
<symbol name="6-PIN-SWD">
<pin name="VDD" direction="pwr"/>
<pin name="RESET" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="SWCLK" direction="in"/>
<pin name="SWDIO"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATSAM4N8A" prefix="U">
<gates>
<gate name="G$1" symbol="ATSAM4N8A"/>
</gates>
<devices>
<device name="ATSAM4N8A" package="LQFP48">
<connects>
<connect gate="G$1" pin="ADVREFP" pad="1"/>
<connect gate="G$1" pin="ERASE/PB12" pad="42"/>
<connect gate="G$1" pin="GND_1" pad="2"/>
<connect gate="G$1" pin="GND_2" pad="34"/>
<connect gate="G$1" pin="JTAGSEL" pad="38"/>
<connect gate="G$1" pin="NRST" pad="29"/>
<connect gate="G$1" pin="PA0/PGMEN0" pad="36"/>
<connect gate="G$1" pin="PA1/PGMEN1" pad="35"/>
<connect gate="G$1" pin="PA10/PGMM2" pad="21"/>
<connect gate="G$1" pin="PA11/PGMM3" pad="20"/>
<connect gate="G$1" pin="PA12/PGMD0" pad="19"/>
<connect gate="G$1" pin="PA13/PGMD1" pad="17"/>
<connect gate="G$1" pin="PA14/PGMD2" pad="16"/>
<connect gate="G$1" pin="PA15/PGMD3" pad="15"/>
<connect gate="G$1" pin="PA16/PGMD4" pad="14"/>
<connect gate="G$1" pin="PA17/PGMD5/AD0" pad="9"/>
<connect gate="G$1" pin="PA18/PGMD6/AD1" pad="10"/>
<connect gate="G$1" pin="PA19/PGMD7/AD2" pad="11"/>
<connect gate="G$1" pin="PA2/PGMEN2" pad="32"/>
<connect gate="G$1" pin="PA20/AD3" pad="12"/>
<connect gate="G$1" pin="PA3" pad="31"/>
<connect gate="G$1" pin="PA5/PGMNCMD" pad="28"/>
<connect gate="G$1" pin="PA5/PGMRDY" pad="27"/>
<connect gate="G$1" pin="PA6/PGMNOE" pad="26"/>
<connect gate="G$1" pin="PA7/XIN32/PGMNVALID" pad="24"/>
<connect gate="G$1" pin="PA8/XOUT32/PGMM0" pad="23"/>
<connect gate="G$1" pin="PA9/PGMM1" pad="22"/>
<connect gate="G$1" pin="PB0/AD4" pad="3"/>
<connect gate="G$1" pin="PB1/AD5" pad="4"/>
<connect gate="G$1" pin="PB10" pad="43"/>
<connect gate="G$1" pin="PB11" pad="44"/>
<connect gate="G$1" pin="PB2/AD6" pad="5"/>
<connect gate="G$1" pin="PB3/AD7" pad="6"/>
<connect gate="G$1" pin="TCK/SWCLK/PB7" pad="40"/>
<connect gate="G$1" pin="TDI/PB4" pad="25"/>
<connect gate="G$1" pin="TDO/TRACESWO/PB5" pad="37"/>
<connect gate="G$1" pin="TMS/SWDIO/PB6" pad="39"/>
<connect gate="G$1" pin="TST" pad="30"/>
<connect gate="G$1" pin="VDDCORE_1" pad="18"/>
<connect gate="G$1" pin="VDDCORE_2" pad="41"/>
<connect gate="G$1" pin="VDDIN" pad="7"/>
<connect gate="G$1" pin="VDDIO_1" pad="13"/>
<connect gate="G$1" pin="VDDIO_2" pad="33"/>
<connect gate="G$1" pin="VDDIO_3" pad="47"/>
<connect gate="G$1" pin="VDDOUT" pad="8"/>
<connect gate="G$1" pin="VDDPLL" pad="48"/>
<connect gate="G$1" pin="XIN/P/PB9/GMCK" pad="46"/>
<connect gate="G$1" pin="XOUT/PB8" pad="45"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSAMS70N-TQFP100" prefix="U">
<gates>
<gate name="G$1" symbol="ATSAMS70N"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="GND3" pad="8"/>
<connect gate="G$1" pin="GND4" pad="10"/>
<connect gate="G$1" pin="GND5" pad="29"/>
<connect gate="G$1" pin="GND6" pad="67"/>
<connect gate="G$1" pin="JTAGSEL" pad="73"/>
<connect gate="G$1" pin="NRST" pad="58"/>
<connect gate="G$1" pin="PA0/I2SC0_MCK" pad="72"/>
<connect gate="G$1" pin="PA1/I2SC0_CK" pad="70"/>
<connect gate="G$1" pin="PA10/UTXD0" pad="46"/>
<connect gate="G$1" pin="PA11/PWMC0_PWMH0" pad="44"/>
<connect gate="G$1" pin="PA12/PWMC0_PWMH1" pad="48"/>
<connect gate="G$1" pin="PA13/PWMC0_PWMH2" pad="27"/>
<connect gate="G$1" pin="PA14/WMC0_PWMH3" pad="34"/>
<connect gate="G$1" pin="PA15/PWMC0_PWML3" pad="33"/>
<connect gate="G$1" pin="PA16/PWMC0_PWML2" pad="30"/>
<connect gate="G$1" pin="PA17/AFE0_AD6" pad="16"/>
<connect gate="G$1" pin="PA18/AFE0_AD7" pad="15"/>
<connect gate="G$1" pin="PA19/PWMC0_PWML0/AFE0_AD8" pad="14"/>
<connect gate="G$1" pin="PA2" pad="66"/>
<connect gate="G$1" pin="PA20/PWMC0_PWML1/AFE0_AD9" pad="13"/>
<connect gate="G$1" pin="PA21/AFE0_AD1" pad="21"/>
<connect gate="G$1" pin="PA22" pad="26"/>
<connect gate="G$1" pin="PA23" pad="31"/>
<connect gate="G$1" pin="PA24" pad="38"/>
<connect gate="G$1" pin="PA25" pad="40"/>
<connect gate="G$1" pin="PA26" pad="42"/>
<connect gate="G$1" pin="PA27" pad="50"/>
<connect gate="G$1" pin="PA28" pad="79"/>
<connect gate="G$1" pin="PA3/TWD0" pad="64"/>
<connect gate="G$1" pin="PA30" pad="82"/>
<connect gate="G$1" pin="PA31/SPI0_NPCS1" pad="83"/>
<connect gate="G$1" pin="PA4/UTXD1/TWCK0" pad="55"/>
<connect gate="G$1" pin="PA5/URXD1" pad="52"/>
<connect gate="G$1" pin="PA7/XIN32" pad="24"/>
<connect gate="G$1" pin="PA8/XOUT32" pad="25"/>
<connect gate="G$1" pin="PA9/URXD0" pad="54"/>
<connect gate="G$1" pin="PB0/RXD0" pad="12"/>
<connect gate="G$1" pin="PB1/TXD0" pad="11"/>
<connect gate="G$1" pin="PB12/ERASE" pad="61"/>
<connect gate="G$1" pin="PB13/DAC0/SCK0" pad="100"/>
<connect gate="G$1" pin="PB2/SPI0_NPCS0/CTS0" pad="17"/>
<connect gate="G$1" pin="PB3/RTS0" pad="20"/>
<connect gate="G$1" pin="PB4/TDI/TWD1" pad="74"/>
<connect gate="G$1" pin="PB5/TDO/TWCK1" pad="77"/>
<connect gate="G$1" pin="PB6/SWDIO/TMS" pad="57"/>
<connect gate="G$1" pin="PB7/SWCLK/TCK" pad="63"/>
<connect gate="G$1" pin="PB8/XOUT" pad="98"/>
<connect gate="G$1" pin="PB9/XIN" pad="99"/>
<connect gate="G$1" pin="PD0/DAC1/PWMC1_PWML0" pad="1"/>
<connect gate="G$1" pin="PD1/PWMC1_PWMH0" pad="92"/>
<connect gate="G$1" pin="PD10/PWMC0_PWML0" pad="71"/>
<connect gate="G$1" pin="PD11/PWMC0_PWMH0" pad="69"/>
<connect gate="G$1" pin="PD12/SPI0_NPCS2" pad="65"/>
<connect gate="G$1" pin="PD13" pad="62"/>
<connect gate="G$1" pin="PD14" pad="59"/>
<connect gate="G$1" pin="PD15" pad="75"/>
<connect gate="G$1" pin="PD16" pad="56"/>
<connect gate="G$1" pin="PD17" pad="53"/>
<connect gate="G$1" pin="PD18/URXD4" pad="49"/>
<connect gate="G$1" pin="PD19/UTXD4" pad="47"/>
<connect gate="G$1" pin="PD2/PWMC1_PWML1" pad="91"/>
<connect gate="G$1" pin="PD20/SPI0_MISO" pad="45"/>
<connect gate="G$1" pin="PD21/SPI0_MOSI" pad="43"/>
<connect gate="G$1" pin="PD22_SPI0_SPCK" pad="41"/>
<connect gate="G$1" pin="PD24" pad="37"/>
<connect gate="G$1" pin="PD25/URXD2" pad="35"/>
<connect gate="G$1" pin="PD26/UTXD2" pad="36"/>
<connect gate="G$1" pin="PD27/SPI0_NPCS3/TWD2" pad="32"/>
<connect gate="G$1" pin="PD28/URXD3/TWCK2" pad="51"/>
<connect gate="G$1" pin="PD3/PWMC1_PWMH1" pad="89"/>
<connect gate="G$1" pin="PD30/UTXD3" pad="23"/>
<connect gate="G$1" pin="PD31" pad="2"/>
<connect gate="G$1" pin="PD4/PWMC1_PWML2" pad="88"/>
<connect gate="G$1" pin="PD5/PWMC1_PWMH2" pad="87"/>
<connect gate="G$1" pin="PD6/PWMC1_PWML3" pad="85"/>
<connect gate="G$1" pin="PD7/PWMC1_PWMH3" pad="84"/>
<connect gate="G$1" pin="PD8" pad="80"/>
<connect gate="G$1" pin="PD9" pad="78"/>
<connect gate="G$1" pin="TST" pad="60"/>
<connect gate="G$1" pin="USB_DM" pad="94"/>
<connect gate="G$1" pin="USB_DP" pad="95"/>
<connect gate="G$1" pin="VBG" pad="97"/>
<connect gate="G$1" pin="VDDCORE1" pad="18"/>
<connect gate="G$1" pin="VDDCORE2" pad="22"/>
<connect gate="G$1" pin="VDDCORE3" pad="39"/>
<connect gate="G$1" pin="VDDCORE4" pad="76"/>
<connect gate="G$1" pin="VDDIN" pad="5"/>
<connect gate="G$1" pin="VDDIO1" pad="19"/>
<connect gate="G$1" pin="VDDIO2" pad="28"/>
<connect gate="G$1" pin="VDDIO3" pad="68"/>
<connect gate="G$1" pin="VDDIO4" pad="81"/>
<connect gate="G$1" pin="VDDOUT" pad="4"/>
<connect gate="G$1" pin="VDDPLL" pad="86"/>
<connect gate="G$1" pin="VDDPLLUSB" pad="90"/>
<connect gate="G$1" pin="VDDUTMIC" pad="96"/>
<connect gate="G$1" pin="VDDUTMII" pad="93"/>
<connect gate="G$1" pin="VREFN" pad="6"/>
<connect gate="G$1" pin="VREFP" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSAMD51">
<gates>
<gate name="G$1" symbol="ATSAMD51"/>
</gates>
<devices>
<device name="QFN64" package="QFN-64-9X9MM">
<connects>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="GND@3" pad="33"/>
<connect gate="G$1" pin="GND@4" pad="47"/>
<connect gate="G$1" pin="GND@5" pad="54"/>
<connect gate="G$1" pin="PA00/SER1-0/TC2-0" pad="1"/>
<connect gate="G$1" pin="PA01/SER1-1/TC2-1" pad="2"/>
<connect gate="G$1" pin="PA02/ADC0-1/DAC-0" pad="3"/>
<connect gate="G$1" pin="PA03/ANAREF-VREFA/ADC0-1" pad="4"/>
<connect gate="G$1" pin="PA04/ANAREF-VREFB/ADC0-4/SER0-0/TC0-0" pad="13"/>
<connect gate="G$1" pin="PA05/ADC0-5/DAC-1/SER0-1/TC0-1" pad="14"/>
<connect gate="G$1" pin="PA06/ANAREF-VREFC/ADC0-6/SER0-2/TC1-0" pad="15"/>
<connect gate="G$1" pin="PA07/ADC0-7/SER0-3/TC1-1" pad="16"/>
<connect gate="G$1" pin="PA08/ADC0-8/ADC1-2/SER0-0/SER2-1/TC0-0" pad="17"/>
<connect gate="G$1" pin="PA09/ADC0-9/ADC1-3/SER0-1/SER2-0/TC0-1" pad="18"/>
<connect gate="G$1" pin="PA10/ADC0-10/SER0-2/SER2-2/TC1-0" pad="19"/>
<connect gate="G$1" pin="PA11/ADC0-11/SER0-3/SER2-3/TC1-1" pad="20"/>
<connect gate="G$1" pin="PA12/SER2-0/SER4-1/TC2-0" pad="29"/>
<connect gate="G$1" pin="PA13/SER2-1/SER4-0/TC2-1" pad="30"/>
<connect gate="G$1" pin="PA14/SER2-2/SER4-2/TC3-0" pad="31"/>
<connect gate="G$1" pin="PA15/SER2-3/SER4-3/TC3-1" pad="32"/>
<connect gate="G$1" pin="PA16/SER1-0/SER3-1/TC2-0" pad="35"/>
<connect gate="G$1" pin="PA17/SER1-1/SER3-0/TC2-1" pad="36"/>
<connect gate="G$1" pin="PA18/SER1-2/SER3-2/TC3-0" pad="37"/>
<connect gate="G$1" pin="PA19/SER1-3/SER3-3/TC3-1" pad="38"/>
<connect gate="G$1" pin="PA20/SER5-2/SER3-2/TC7-0" pad="41"/>
<connect gate="G$1" pin="PA21/SER5-3/SER3-3/TC7-1" pad="42"/>
<connect gate="G$1" pin="PA22/SER3-0/SER5-1/TC4-0" pad="43"/>
<connect gate="G$1" pin="PA23/SER3-1/SER5-0/TC4-1" pad="44"/>
<connect gate="G$1" pin="PA24/SER3-2/SER5-2/TC5-0/USBDM" pad="45"/>
<connect gate="G$1" pin="PA25/SER3-3/SER5-3/TC5-1/USBDP" pad="46"/>
<connect gate="G$1" pin="PA27/GCLK-1" pad="51"/>
<connect gate="G$1" pin="PA30/SER7-2/SER1-2/TC6-0/SWCLK" pad="57"/>
<connect gate="G$1" pin="PA31/SER7-3/SER1-3/TC6-1" pad="58"/>
<connect gate="G$1" pin="PB00/ADC0-12/SER5-2/TC7-0" pad="61"/>
<connect gate="G$1" pin="PB01/ADC0-13/SER5-3/TC7-1" pad="62"/>
<connect gate="G$1" pin="PB02/ADC0-14/SER5-0/TC6-0" pad="63"/>
<connect gate="G$1" pin="PB03/ADC0/SER5-1/TC6" pad="64"/>
<connect gate="G$1" pin="PB04/ADC1-6" pad="5"/>
<connect gate="G$1" pin="PB05/ADC1-7" pad="6"/>
<connect gate="G$1" pin="PB06/ADC1-8" pad="9"/>
<connect gate="G$1" pin="PB07/ADC1-9" pad="10"/>
<connect gate="G$1" pin="PB08/ADC0-2/ADC1-9/SER4-0/TC4-0" pad="11"/>
<connect gate="G$1" pin="PB09/ADC0-3/ADC1-1/SE4-1/TC4-1" pad="12"/>
<connect gate="G$1" pin="PB10/SER4-2/TC5-0" pad="23"/>
<connect gate="G$1" pin="PB11/SER4-3/TC5-1" pad="24"/>
<connect gate="G$1" pin="PB12/SER4-0/TC4-0" pad="25"/>
<connect gate="G$1" pin="PB13/SER4-1/TC4-1" pad="26"/>
<connect gate="G$1" pin="PB14/SER4-2/TC5-0" pad="27"/>
<connect gate="G$1" pin="PB15/SER4-3/TC5-1" pad="28"/>
<connect gate="G$1" pin="PB16/SER5-0/TC6-0" pad="39"/>
<connect gate="G$1" pin="PB17/SER5-1/TC6-1" pad="40"/>
<connect gate="G$1" pin="PB22/SER1-2/SER5-2/TC7-0" pad="49"/>
<connect gate="G$1" pin="PB23/SER1-3/SER5-3/TC7-1" pad="50"/>
<connect gate="G$1" pin="PB30/SER7-0/SER5-1/TC0-0/SWDIO" pad="59"/>
<connect gate="G$1" pin="PB31/SER7-1/SER5-0/TC0-1" pad="60"/>
<connect gate="G$1" pin="RESETN" pad="52"/>
<connect gate="G$1" pin="VDDANA" pad="8"/>
<connect gate="G$1" pin="VDDCORE" pad="53"/>
<connect gate="G$1" pin="VDDIO@1" pad="21"/>
<connect gate="G$1" pin="VDDIO@2" pad="34"/>
<connect gate="G$1" pin="VDDIO@3" pad="48"/>
<connect gate="G$1" pin="VDDIO@4" pad="56"/>
<connect gate="G$1" pin="VSW" pad="55"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC2030-SWD" prefix="J" uservalue="yes">
<description>&lt;h3&gt;TAG-CONNECT ICSP Connector&lt;/h3&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="http://www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.&lt;BR&gt;
Two variants - one "with legs" (for hands-free fit on PCB) and another "without legs" for quick programming.

&lt;p&gt;
&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
<gates>
<gate name="G$1" symbol="6-PIN-SWD"/>
</gates>
<devices>
<device name="-MCP" package="TC2030-MCP">
<connects>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SWCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="6"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MCP-NL" package="TC2030-MCP-NL">
<connects>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SWCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="6"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TC2030-MCP-NL-CP">
<connects>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SWCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="6"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
