<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.1">
<drawing>
<library>
<packages>
<package name="RJ12-6-SMT">
</package>
<package name="RJ12-6-SMT-WIDE">
</package>
<package name="JST-6-SMD-HORI-1.0MM">
<description>&lt;h3&gt;JST SH Vertical 6-Pin SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 1 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;JST_6PIN_VERTICAL&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="RJ12-6-SMT-TOPENTRY">
</package>
<package name="JRTOMBSTONE">
</package>
<package name="RJ12-6-SMT-NOSILK">
</package>
<package name="RASPBERRYPI-3BPLUS">
</package>
<package name="POGO">
</package>
<package name="DX4R005HJ5_100">
</package>
<package name="DX4R005HJ5">
</package>
<package name="DX4R005HJ5_64">
</package>
<package name="MK-LOGO-SILK">
</package>
<package name="CBA-SILK-LOGO">
</package>
<package name="RJ45-LED-RJE7318800XXX">
</package>
<package name="SJFAB">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="RJ45-LED-RJHSE-5381-UPTAB">
</package>
</packages>
<symbols>
<symbol name="RJ12-6">
<pin name="1"/>
<pin name="3"/>
<pin name="5"/>
<pin name="2"/>
<pin name="4"/>
<pin name="6"/>
</symbol>
<symbol name="CONN_06">
<description>&lt;h3&gt;6 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="CONN_02">
<description>&lt;h3&gt;2 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JRTOMBSTONE">
</symbol>
<symbol name="RASPBERRY-PI-3-BPLUS">
</symbol>
<symbol name="POGO">
<pin name="POGO"/>
</symbol>
<symbol name="USB-1">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="ATK-PHY">
<pin name="TX"/>
<pin name="RX"/>
<pin name="CLKIN"/>
<pin name="GND"/>
<pin name="3V3"/>
<pin name="GRN-RX"/>
<pin name="YLW-TX"/>
<pin name="CLKOUT"/>
</symbol>
<symbol name="SJFAB">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="DOT">
</symbol>
<symbol name="ATK-RS48PHYVE">
<pin name="3V3-LED"/>
<pin name="LED-GRN-CATHODE"/>
<pin name="LED-YLW-CATHODE"/>
<pin name="CLKRX-Y"/>
<pin name="CLKTX-Z"/>
<pin name="RX-A"/>
<pin name="RX-B"/>
<pin name="TX-Z"/>
<pin name="TX-Y"/>
<pin name="CLKRX-B"/>
<pin name="CLKRX-A"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RJ12-6-SMT" prefix="J">
<gates>
<gate name="G$1" symbol="RJ12-6"/>
</gates>
<devices>
<device name="" package="RJ12-6-SMT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="RJ12-6-SMT-WIDE">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOP" package="RJ12-6-SMT-TOPENTRY">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOSILK" package="RJ12-6-SMT-NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_6_PIN_HORIZONTAL" prefix="J">
<description>&lt;h3&gt;JST 6 pin horizontal connector&lt;/h3&gt;
JST-SH type.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="link"&gt;name&lt;/a&gt; (XXX-00000)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was used on these SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="link"&gt;name&lt;/a&gt; (XXX-00000)&lt;/li&gt;
&lt;li&gt;&lt;a href="link"&gt;name&lt;/a&gt; (XXX-00000)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="A" symbol="CONN_06"/>
</gates>
<devices>
<device name="" package="JST-6-SMD-HORI-1.0MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE" value="BM06B-SRSS-TB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JRTOMBSTONE" prefix="MP">
<gates>
<gate name="G$1" symbol="JRTOMBSTONE"/>
</gates>
<devices>
<device name="" package="JRTOMBSTONE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPBERRYPI-3BPLUS" prefix="U">
<gates>
<gate name="G$1" symbol="RASPBERRY-PI-3-BPLUS"/>
</gates>
<devices>
<device name="" package="RASPBERRYPI-3BPLUS">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POGO" prefix="J">
<gates>
<gate name="G$1" symbol="POGO"/>
</gates>
<devices>
<device name="" package="POGO">
<connects>
<connect gate="G$1" pin="POGO" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO-USB" prefix="X">
<description>SMD micro USB connector as found in the fablab inventory. 
Three footprint variants included: 
&lt;ol&gt;
&lt;li&gt; original, as described by manufacturer's datasheet
&lt;li&gt; for milling with the 1/100" bit
&lt;li&gt; for milling with the 1/64" bit
&lt;/ol&gt;
&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="USB-1"/>
</gates>
<devices>
<device name="_1/100" package="DX4R005HJ5_100">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_ORIG" package="DX4R005HJ5">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1/64" package="DX4R005HJ5_64">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MK-LOGO">
<gates>
</gates>
<devices>
<device name="" package="MK-LOGO-SILK">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CBA-LOGO">
<gates>
</gates>
<devices>
<device name="" package="CBA-SILK-LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATK-PHY" prefix="J">
<gates>
<gate name="G$1" symbol="ATK-PHY"/>
</gates>
<devices>
<device name="" package="RJ45-LED-RJE7318800XXX">
<connects>
<connect gate="G$1" pin="3V3" pad="GRNP P$4 P$5 YLWP"/>
<connect gate="G$1" pin="CLKIN" pad="P$1"/>
<connect gate="G$1" pin="CLKOUT" pad="P$8"/>
<connect gate="G$1" pin="GND" pad="P$2 P$7 SHDL1 SHDL2"/>
<connect gate="G$1" pin="GRN-RX" pad="GRNN"/>
<connect gate="G$1" pin="RX" pad="P$3"/>
<connect gate="G$1" pin="TX" pad="P$6"/>
<connect gate="G$1" pin="YLW-TX" pad="YLWN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDER_JUMPER" prefix="J">
<gates>
<gate name="G$1" symbol="SJFAB"/>
</gates>
<devices>
<device name="" package="SJFAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL" prefix="J">
<description>For use by pick and place machines to calibrate the vision/machine, 1mm
&lt;p&gt;By microbuilder.eu&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DOT"/>
</gates>
<devices>
<device name="" package="FIDUCIAL_1MM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATK-RS48PHYVE" prefix="J">
<gates>
<gate name="G$1" symbol="ATK-RS48PHYVE"/>
</gates>
<devices>
<device name="RJ45LED" package="RJ45-LED-RJE7318800XXX">
<connects>
<connect gate="G$1" pin="3V3-LED" pad="GRNP YLWP"/>
<connect gate="G$1" pin="CLKRX-A" pad="P$8"/>
<connect gate="G$1" pin="CLKRX-B" pad="P$7"/>
<connect gate="G$1" pin="CLKRX-Y" pad="P$1"/>
<connect gate="G$1" pin="CLKTX-Z" pad="P$2"/>
<connect gate="G$1" pin="LED-GRN-CATHODE" pad="GRNN"/>
<connect gate="G$1" pin="LED-YLW-CATHODE" pad="YLWN"/>
<connect gate="G$1" pin="RX-A" pad="P$3"/>
<connect gate="G$1" pin="RX-B" pad="P$4"/>
<connect gate="G$1" pin="TX-Y" pad="P$6"/>
<connect gate="G$1" pin="TX-Z" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ45LEDTABUP" package="RJ45-LED-RJHSE-5381-UPTAB">
<connects>
<connect gate="G$1" pin="3V3-LED" pad="GRNP YLWP"/>
<connect gate="G$1" pin="CLKRX-A" pad="P$8"/>
<connect gate="G$1" pin="CLKRX-B" pad="P$7"/>
<connect gate="G$1" pin="CLKRX-Y" pad="P$1"/>
<connect gate="G$1" pin="CLKTX-Z" pad="P$2"/>
<connect gate="G$1" pin="LED-GRN-CATHODE" pad="GRNN"/>
<connect gate="G$1" pin="LED-YLW-CATHODE" pad="YLWN"/>
<connect gate="G$1" pin="RX-A" pad="P$3"/>
<connect gate="G$1" pin="RX-B" pad="P$4"/>
<connect gate="G$1" pin="TX-Y" pad="P$6"/>
<connect gate="G$1" pin="TX-Z" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
