<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<library>
<description>&lt;b&gt;Infineon Technologies&lt;/b&gt;&lt;p&gt;
http://www.infineon.comp&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P-TSSOP28-1">
<description>Infineon &lt;b&gt;P-TSSOP-28-1&lt;/b&gt;&lt;p&gt;
TDA 6060 XS cross-ref_pFET-60v_p_chan.pdf</description>
</package>
<package name="TO252-5-11">
<description>&lt;b&gt;Dpak-5 Pin&lt;/b&gt; P-TO252-5-11 &lt;/b&gt;&lt;p&gt;
Source: www.infineon.com .. BTS428L2_20030912.pdf</description>
</package>
<package name="LOGO">
<description>&lt;b&gt;Infineon Logo&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TO220-51">
<description>&lt;b&gt;TO-218AB/5-1&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/upload/Document/cmc_upload/documents/011/8726/Datasheet_BTS555.pdf</description>
</package>
<package name="TO220-52">
<description>&lt;b&gt;TO-218AB/5 Option E3146&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/upload/Document/cmc_upload/documents/011/8726/Datasheet_BTS555.pdf</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="PG-DSO-36">
<description>&lt;b&gt;Smart Power High-Side-Switch for Industrial Applications. Eight Channels: 8 x 200 m?&lt;/b&gt;&lt;p&gt;
PG-DSO-36&lt;br&gt;
Source: http://www.infineon.com .. ITS4880R_20060309.pdf</description>
</package>
<package name="PG-DSO-36W">
<description>&lt;b&gt;PG-DSO-36 Wave&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. ITS4880R_20060309.pdf</description>
</package>
<package name="PG-DSO-36PAD">
<description>PG-DSO-36&lt;br&gt; with thermal on top and bottom&lt;p&gt;
Source: http://www.infineon.com .. ITS4880R_20060309.pdf</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="PG-VQFN-108-2">
<description>&lt;b&gt;PG-VQFN-108-2&lt;/b&gt;&lt;p&gt;
Source: Z8B00137584_POL_PG_VQFN_108_2_02.pdf</description>
</package>
<package name="P-TO220-7-12">
<description>&lt;b&gt;Plastic Transistor Single Outline Package&lt;/b&gt;P-TO220-7-12&lt;p&gt;
Source: http://www.infineon.com .. tle5205-2.pdf</description>
</package>
<package name="P-TO263-7-1">
<description>&lt;b&gt;Plastic Transistor Single Outline Package&lt;/b&gt; P-TO263-7-1 Option E3180&lt;p&gt;


Source: http://www.infineon.com .. tle5205-2.pdf</description>
</package>
<package name="P-TO220-7-11">
<description>&lt;b&gt;(Plastic Transistor Single Outline Package)&lt;/b&gt;P-TO220-7-11&lt;p&gt;
Source: http://www.infineon.com .. tle5205-2.pdf</description>
</package>
<package name="PG-DSO-20">
<description>&lt;b&gt;PG-DSO-20&lt;/b&gt; Plastic Dual Small Outline Package&lt;p&gt;
Source: http://www.infineon.com/products .. BTS176G.pdf</description>
</package>
<package name="PG-SOT-223">
<description>&lt;b&gt;Small Outline Transistor; 4 leads&lt;/b&gt; Wave soldering&lt;p&gt;
Source: http://www.infineon.com/dgdl/BSP613P_Rev2.4.pdf</description>
</package>
<package name="SC74_INFINEON">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt; Reflow soldering&lt;p&gt;
INFINEON, www.infineon.com/cmc_upload/0/000/010/257/eh_db_5b.pdf</description>
</package>
<package name="PG-DSO-8">
<description>&lt;b&gt;PG-DSO8&lt;/b&gt;&lt;p&gt;
Source: TLE5009_FDS_Rev.1.1.pdf</description>
</package>
<package name="PG-TO263-7-3">
<description>&lt;b&gt;PG-TO263-7-3&lt;/b&gt;&lt;p&gt;
Source: 1859075.pdf (Farnell)</description>
</package>
<package name="DIRECT-FET-ME">
</package>
<package name="PQFN">
</package>
</packages>
<symbols>
<symbol name="TDA6060">
<pin name="AUDGND" direction="pwr"/>
<pin name="AUDINFM" direction="in"/>
<pin name="AUDINAM" direction="in"/>
<pin name="SC2IN" direction="in"/>
<pin name="CAS" direction="in"/>
<pin name="MODOUT1" direction="out"/>
<pin name="MODGND" direction="pwr"/>
<pin name="MODOUT2" direction="out"/>
<pin name="GNDD" direction="pwr"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="VCCD" direction="pwr"/>
<pin name="Q" direction="pas"/>
<pin name="QX" direction="pas"/>
<pin name="P2/ADC" direction="in"/>
<pin name="CHGPMP" direction="in"/>
<pin name="VTUNE" direction="in"/>
<pin name="T1" direction="in"/>
<pin name="O-B1" direction="in"/>
<pin name="O-C2" direction="pas"/>
<pin name="O-C1" direction="pas"/>
<pin name="O-B2" direction="in"/>
<pin name="GNDA" direction="pwr"/>
<pin name="VIDIN" direction="in"/>
<pin name="SLF" direction="pas"/>
<pin name="TFLF" direction="pas"/>
<pin name="T2" direction="pas"/>
<pin name="VCCA" direction="pwr"/>
</symbol>
<symbol name="BTS428L2">
<pin name="IN" direction="in"/>
<pin name="ST" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="BTS555">
<pin name="IN" direction="in"/>
<pin name="IS" direction="pas"/>
<pin name="VBB" direction="pas"/>
<pin name="O1" direction="pas"/>
<pin name="O2" direction="pas"/>
</symbol>
<symbol name="TCA965">
<pin name="V7" direction="in"/>
<pin name="V8" direction="in"/>
<pin name="V9" direction="in"/>
<pin name="V6" direction="in"/>
<pin name="B" direction="oc"/>
<pin name="INH_B" direction="in"/>
<pin name="D" direction="oc"/>
<pin name="C" direction="oc"/>
<pin name="INH_A" direction="in"/>
<pin name="A" direction="oc"/>
<pin name="VSTAB" direction="out"/>
<pin name="VREF" direction="pas"/>
<pin name="+V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ITS4880R">
<pin name="DIAG" direction="out"/>
<pin name="LS" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="VBB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VBB@1" direction="in"/>
<pin name="OUT1@2" direction="out"/>
<pin name="OUT2@2" direction="out"/>
<pin name="OUT3@2" direction="out"/>
<pin name="OUT4@2" direction="out"/>
<pin name="OUT5@2" direction="out"/>
<pin name="OUT6@2" direction="out"/>
<pin name="OUT7@2" direction="out"/>
<pin name="OUT8@2" direction="out"/>
</symbol>
<symbol name="ITS4880R-W">
<pin name="DIAG" direction="out"/>
<pin name="LS" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="VBB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VBB@1" direction="in"/>
<pin name="OUT1@2" direction="out"/>
<pin name="OUT2@2" direction="out"/>
<pin name="OUT3@2" direction="out"/>
<pin name="OUT4@2" direction="out"/>
<pin name="OUT5@2" direction="out"/>
<pin name="OUT6@2" direction="out"/>
<pin name="OUT7@2" direction="out"/>
<pin name="OUT8@2" direction="out"/>
<pin name="VBB@2" direction="in"/>
</symbol>
<symbol name="VBB">
<pin name="VBB" direction="in"/>
</symbol>
<symbol name="VBB10">
<pin name="VBB@1" direction="pas"/>
<pin name="VBB@2" direction="pas"/>
<pin name="VBB@3" direction="pas"/>
<pin name="VBB@4" direction="pas"/>
<pin name="VBB@5" direction="pas"/>
<pin name="VBB@6" direction="pas"/>
<pin name="VBB@7" direction="pas"/>
<pin name="VBB@8" direction="pas"/>
<pin name="VBB@9" direction="pas"/>
<pin name="VBB@10" direction="pas"/>
</symbol>
<symbol name="TCA785">
<pin name="GND" direction="pwr"/>
<pin name="!Q2" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="QU" direction="out"/>
<pin name="QZ" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="!Q1" direction="out"/>
<pin name="I" direction="in"/>
<pin name="VSYNC" direction="in"/>
<pin name="R9" direction="in"/>
<pin name="C10" direction="in"/>
<pin name="L" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="V11" direction="in"/>
<pin name="C12" direction="in"/>
</symbol>
<symbol name="TLE5205-2">
<pin name="EF" direction="oc"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="VS" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="BTS716G">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="GND3/4" direction="in"/>
<pin name="GND1/2" direction="in"/>
<pin name="ST1/2" direction="in"/>
<pin name="ST3/4" direction="in"/>
</symbol>
<symbol name="VBB8">
<pin name="VBB@1" direction="pwr"/>
<pin name="VBB@2" direction="pwr"/>
<pin name="VBB@3" direction="pwr"/>
<pin name="VBB@4" direction="pwr"/>
<pin name="VBB@5" direction="pwr"/>
<pin name="VBB@6" direction="pwr"/>
<pin name="VBB@7" direction="pwr"/>
<pin name="VBB@8" direction="pwr"/>
</symbol>
<symbol name="P-SIPMOS-2D">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D@1" direction="pas"/>
<pin name="D@2" direction="pas"/>
</symbol>
<symbol name="P-SIPMOS">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="ILD4001">
<pin name="VS" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="EN/PWM" direction="in"/>
<pin name="VSENSE" direction="in"/>
<pin name="VDRIVE" direction="out"/>
</symbol>
<symbol name="TLE5009">
<pin name="COS_P" direction="out"/>
<pin name="COS_N" direction="out"/>
<pin name="SIN_P" direction="out"/>
<pin name="SIN_N" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VGMR" direction="pas"/>
</symbol>
<symbol name="NMOS-FET-E">
<description>MOSFET N-channel - Enhancement mode</description>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRF7580">
<description>MOSFET N-channel - Enhancement mode</description>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRF7480">
<description>MOSFET N-channel - Enhancement mode</description>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRLHS2242TR">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TDA6060*" prefix="IC">
<description>&lt;b&gt;Phase locked loop&lt;/b&gt;&lt;p&gt;
(PLL), with a multistandard video modulator and a&lt;p&gt;
programmable sound FM and AM modulator</description>
<gates>
<gate name="G$1" symbol="TDA6060"/>
</gates>
<devices>
<device name="" package="P-TSSOP28-1">
<connects>
<connect gate="G$1" pin="AUDGND" pad="1"/>
<connect gate="G$1" pin="AUDINAM" pad="3"/>
<connect gate="G$1" pin="AUDINFM" pad="2"/>
<connect gate="G$1" pin="CAS" pad="5"/>
<connect gate="G$1" pin="CHGPMP" pad="16"/>
<connect gate="G$1" pin="GNDA" pad="23"/>
<connect gate="G$1" pin="GNDD" pad="9"/>
<connect gate="G$1" pin="MODGND" pad="7"/>
<connect gate="G$1" pin="MODOUT1" pad="6"/>
<connect gate="G$1" pin="MODOUT2" pad="8"/>
<connect gate="G$1" pin="O-B1" pad="19"/>
<connect gate="G$1" pin="O-B2" pad="22"/>
<connect gate="G$1" pin="O-C1" pad="21"/>
<connect gate="G$1" pin="O-C2" pad="20"/>
<connect gate="G$1" pin="P2/ADC" pad="15"/>
<connect gate="G$1" pin="Q" pad="13"/>
<connect gate="G$1" pin="QX" pad="14"/>
<connect gate="G$1" pin="SC2IN" pad="4"/>
<connect gate="G$1" pin="SCL" pad="11"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="SLF" pad="25"/>
<connect gate="G$1" pin="T1" pad="18"/>
<connect gate="G$1" pin="T2" pad="27"/>
<connect gate="G$1" pin="TFLF" pad="26"/>
<connect gate="G$1" pin="VCCA" pad="28"/>
<connect gate="G$1" pin="VCCD" pad="12"/>
<connect gate="G$1" pin="VIDIN" pad="24"/>
<connect gate="G$1" pin="VTUNE" pad="17"/>
</connects>
<technologies>
<technology name="G">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="XS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTS428L2" prefix="IC">
<description>&lt;b&gt;Smart High-Side Power Switch&lt;/b&gt;&lt;p&gt;
One Channel: 60mOhm Status Feedback&lt;br&gt;
Source: Source: www.infineon.com .. BTS428L2_20030912.pdf</description>
<gates>
<gate name="G$1" symbol="BTS428L2"/>
</gates>
<devices>
<device name="" package="TO252-5-11">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="ST" pad="4"/>
<connect gate="G$1" pin="VBB" pad="TAB"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTS555" prefix="IC">
<description>&lt;b&gt;PROFET® Data Sheet BTS555&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/upload/Document/cmc_upload/documents/011/8726/Datasheet_BTS555.pdf</description>
<gates>
<gate name="G$1" symbol="BTS555"/>
</gates>
<devices>
<device name="" package="TO220-51">
<connects>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="IS" pad="4"/>
<connect gate="G$1" pin="O1" pad="1"/>
<connect gate="G$1" pin="O2" pad="5"/>
<connect gate="G$1" pin="VBB" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="BTS555."/>
<attribute name="OC_FARNELL" value="4109260"/>
<attribute name="OC_NEWARK" value="26H6766"/>
</technology>
</technologies>
</device>
<device name="E3146" package="TO220-52">
<connects>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="IS" pad="4"/>
<connect gate="G$1" pin="O1" pad="1"/>
<connect gate="G$1" pin="O2" pad="5"/>
<connect gate="G$1" pin="VBB" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCA965" prefix="IC">
<description>&lt;b&gt;Window Discriminator&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/upload/Document/cmc_upload/documents/012/1090/tca965b_green_050217.pdf</description>
<gates>
<gate name="G$1" symbol="TCA965"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+V" pad="11"/>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="INH_A" pad="4"/>
<connect gate="G$1" pin="INH_B" pad="12"/>
<connect gate="G$1" pin="V6" pad="6"/>
<connect gate="G$1" pin="V7" pad="7"/>
<connect gate="G$1" pin="V8" pad="8"/>
<connect gate="G$1" pin="V9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="5"/>
<connect gate="G$1" pin="VSTAB" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITS4880R" prefix="IC">
<description>&lt;b&gt;Smart Power High-Side-Switch for Industrial Applications. Eight Channels: 8 x 200 mOhm&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. ITS4880R_20060309.pdf</description>
<gates>
<gate name="G$1" symbol="ITS4880R"/>
</gates>
<devices>
<device name="" package="PG-DSO-36">
<connects>
<connect gate="G$1" pin="DIAG" pad="20"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="IN1" pad="6"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="8"/>
<connect gate="G$1" pin="IN4" pad="9"/>
<connect gate="G$1" pin="IN5" pad="10"/>
<connect gate="G$1" pin="IN6" pad="11"/>
<connect gate="G$1" pin="IN7" pad="12"/>
<connect gate="G$1" pin="IN8" pad="13"/>
<connect gate="G$1" pin="LS" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="36"/>
<connect gate="G$1" pin="OUT1@2" pad="35"/>
<connect gate="G$1" pin="OUT2" pad="34"/>
<connect gate="G$1" pin="OUT2@2" pad="33"/>
<connect gate="G$1" pin="OUT3" pad="32"/>
<connect gate="G$1" pin="OUT3@2" pad="31"/>
<connect gate="G$1" pin="OUT4" pad="30"/>
<connect gate="G$1" pin="OUT4@2" pad="29"/>
<connect gate="G$1" pin="OUT5" pad="28"/>
<connect gate="G$1" pin="OUT5@2" pad="27"/>
<connect gate="G$1" pin="OUT6" pad="26"/>
<connect gate="G$1" pin="OUT6@2" pad="25"/>
<connect gate="G$1" pin="OUT7" pad="24"/>
<connect gate="G$1" pin="OUT7@2" pad="23"/>
<connect gate="G$1" pin="OUT8" pad="22"/>
<connect gate="G$1" pin="OUT8@2" pad="21"/>
<connect gate="G$1" pin="VBB" pad="TH@1"/>
<connect gate="G$1" pin="VBB@1" pad="TH@2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ITS4880R"/>
<attribute name="OC_FARNELL" value="1440818"/>
<attribute name="OC_NEWARK" value="58M7534"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITS4880R-W" prefix="IC">
<description>&lt;b&gt;Smart Power High-Side-Switch for Industrial Applications. Eight Channels: 8 x 200 mOhm&lt;/b&gt;&lt;p&gt;
with pad for hand soldering&lt;br&gt;
Source: http://www.infineon.com .. ITS4880R_20060309.pdf</description>
<gates>
<gate name="G$1" symbol="ITS4880R-W"/>
</gates>
<devices>
<device name="" package="PG-DSO-36W">
<connects>
<connect gate="G$1" pin="DIAG" pad="20"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="IN1" pad="6"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="8"/>
<connect gate="G$1" pin="IN4" pad="9"/>
<connect gate="G$1" pin="IN5" pad="10"/>
<connect gate="G$1" pin="IN6" pad="11"/>
<connect gate="G$1" pin="IN7" pad="12"/>
<connect gate="G$1" pin="IN8" pad="13"/>
<connect gate="G$1" pin="LS" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="36"/>
<connect gate="G$1" pin="OUT1@2" pad="35"/>
<connect gate="G$1" pin="OUT2" pad="34"/>
<connect gate="G$1" pin="OUT2@2" pad="33"/>
<connect gate="G$1" pin="OUT3" pad="32"/>
<connect gate="G$1" pin="OUT3@2" pad="31"/>
<connect gate="G$1" pin="OUT4" pad="30"/>
<connect gate="G$1" pin="OUT4@2" pad="29"/>
<connect gate="G$1" pin="OUT5" pad="28"/>
<connect gate="G$1" pin="OUT5@2" pad="27"/>
<connect gate="G$1" pin="OUT6" pad="26"/>
<connect gate="G$1" pin="OUT6@2" pad="25"/>
<connect gate="G$1" pin="OUT7" pad="24"/>
<connect gate="G$1" pin="OUT7@2" pad="23"/>
<connect gate="G$1" pin="OUT8" pad="22"/>
<connect gate="G$1" pin="OUT8@2" pad="21"/>
<connect gate="G$1" pin="VBB" pad="TH@1"/>
<connect gate="G$1" pin="VBB@1" pad="TH@2"/>
<connect gate="G$1" pin="VBB@2" pad="TH@3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITS4880R-PAD" prefix="IC">
<description>&lt;b&gt;Smart Power High-Side-Switch for Industrial Applications. Eight Channels: 8 x 200 mOhm&lt;/b&gt;&lt;p&gt;
with thermal pad to bottom side&lt;br&gt;
Source: http://www.infineon.com .. ITS4880R_20060309.pdf</description>
<gates>
<gate name="''" symbol="ITS4880R"/>
<gate name="P1" symbol="VBB10"/>
</gates>
<devices>
<device name="" package="PG-DSO-36PAD">
<connects>
<connect gate="''" pin="DIAG" pad="20"/>
<connect gate="''" pin="GND" pad="19"/>
<connect gate="''" pin="IN1" pad="6"/>
<connect gate="''" pin="IN2" pad="7"/>
<connect gate="''" pin="IN3" pad="8"/>
<connect gate="''" pin="IN4" pad="9"/>
<connect gate="''" pin="IN5" pad="10"/>
<connect gate="''" pin="IN6" pad="11"/>
<connect gate="''" pin="IN7" pad="12"/>
<connect gate="''" pin="IN8" pad="13"/>
<connect gate="''" pin="LS" pad="3"/>
<connect gate="''" pin="OUT1" pad="36"/>
<connect gate="''" pin="OUT1@2" pad="35"/>
<connect gate="''" pin="OUT2" pad="34"/>
<connect gate="''" pin="OUT2@2" pad="33"/>
<connect gate="''" pin="OUT3" pad="32"/>
<connect gate="''" pin="OUT3@2" pad="31"/>
<connect gate="''" pin="OUT4" pad="30"/>
<connect gate="''" pin="OUT4@2" pad="29"/>
<connect gate="''" pin="OUT5" pad="28"/>
<connect gate="''" pin="OUT5@2" pad="27"/>
<connect gate="''" pin="OUT6" pad="26"/>
<connect gate="''" pin="OUT6@2" pad="25"/>
<connect gate="''" pin="OUT7" pad="24"/>
<connect gate="''" pin="OUT7@2" pad="23"/>
<connect gate="''" pin="OUT8" pad="22"/>
<connect gate="''" pin="OUT8@2" pad="21"/>
<connect gate="''" pin="VBB" pad="TH@1"/>
<connect gate="''" pin="VBB@1" pad="TH@2"/>
<connect gate="P1" pin="VBB@1" pad="TH@3"/>
<connect gate="P1" pin="VBB@10" pad="TH@12"/>
<connect gate="P1" pin="VBB@2" pad="TH@4"/>
<connect gate="P1" pin="VBB@3" pad="TH@5"/>
<connect gate="P1" pin="VBB@4" pad="TH@6"/>
<connect gate="P1" pin="VBB@5" pad="TH@7"/>
<connect gate="P1" pin="VBB@6" pad="TH@8"/>
<connect gate="P1" pin="VBB@7" pad="TH@9"/>
<connect gate="P1" pin="VBB@8" pad="TH@10"/>
<connect gate="P1" pin="VBB@9" pad="TH@11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCA785" prefix="IC">
<description>&lt;b&gt;Phase Control IC&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/ .. tca785.pdf</description>
<gates>
<gate name="P1" symbol="TCA785"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="P1" pin="!Q1" pad="4"/>
<connect gate="P1" pin="!Q2" pad="2"/>
<connect gate="P1" pin="C10" pad="10"/>
<connect gate="P1" pin="C12" pad="12"/>
<connect gate="P1" pin="GND" pad="1"/>
<connect gate="P1" pin="I" pad="6"/>
<connect gate="P1" pin="L" pad="13"/>
<connect gate="P1" pin="Q1" pad="14"/>
<connect gate="P1" pin="Q2" pad="15"/>
<connect gate="P1" pin="QU" pad="3"/>
<connect gate="P1" pin="QZ" pad="7"/>
<connect gate="P1" pin="R9" pad="9"/>
<connect gate="P1" pin="V11" pad="11"/>
<connect gate="P1" pin="VREF" pad="8"/>
<connect gate="P1" pin="VS" pad="16"/>
<connect gate="P1" pin="VSYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLE5205-2" prefix="IC">
<description>&lt;b&gt;5-A H-Bridge for DC-Motor Applications&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. tle5205-2.pdf</description>
<gates>
<gate name="G$1" symbol="TLE5205-2"/>
</gates>
<devices>
<device name="" package="P-TO220-7-11">
<connects>
<connect gate="G$1" pin="EF" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="G" package="P-TO263-7-1">
<connects>
<connect gate="G$1" pin="EF" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="P-TO220-7-12">
<connects>
<connect gate="G$1" pin="EF" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTS716G" prefix="IC">
<description>&lt;b&gt;Smart High-Side Power Switch Four Channels: 4 x 140mOhm staus Feedback&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/dgdl/BTS716G.pdf</description>
<gates>
<gate name="G$1" symbol="BTS716G"/>
<gate name="G$2" symbol="VBB8"/>
</gates>
<devices>
<device name="" package="PG-DSO-20">
<connects>
<connect gate="G$1" pin="GND1/2" pad="2"/>
<connect gate="G$1" pin="GND3/4" pad="6"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="7"/>
<connect gate="G$1" pin="IN4" pad="9"/>
<connect gate="G$1" pin="OUT1" pad="18"/>
<connect gate="G$1" pin="OUT2" pad="17"/>
<connect gate="G$1" pin="OUT3" pad="14"/>
<connect gate="G$1" pin="OUT4" pad="13"/>
<connect gate="G$1" pin="ST1/2" pad="4"/>
<connect gate="G$1" pin="ST3/4" pad="8"/>
<connect gate="G$2" pin="VBB@1" pad="1"/>
<connect gate="G$2" pin="VBB@2" pad="10"/>
<connect gate="G$2" pin="VBB@3" pad="11"/>
<connect gate="G$2" pin="VBB@4" pad="12"/>
<connect gate="G$2" pin="VBB@5" pad="15"/>
<connect gate="G$2" pin="VBB@6" pad="16"/>
<connect gate="G$2" pin="VBB@7" pad="19"/>
<connect gate="G$2" pin="VBB@8" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BSP613P" prefix="Q">
<description>&lt;b&gt;SIPMOS (R) Small-Signal-Transistor&lt;/b&gt; P-Channel (2 Drain)&lt;p&gt;
Source: http://www.infineon.com/dgdl/BSP613P_Rev2.4.pdf</description>
<gates>
<gate name="G$1" symbol="P-SIPMOS-2D"/>
</gates>
<devices>
<device name="" package="PG-SOT-223">
<connects>
<connect gate="G$1" pin="D@1" pad="2"/>
<connect gate="G$1" pin="D@2" pad="4"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ILD4001" prefix="IC">
<description>&lt;b&gt;LED Driver for High Power LEDs&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/dgdl/ILD4001-Step-down-LED-Controller-Rev2.0.pdf?folderId=db3a30431f848401011fcbf2ab4c04c4&amp;fileId=db3a30433072cd8f01308fc1af03786b</description>
<gates>
<gate name="G$1" symbol="ILD4001"/>
</gates>
<devices>
<device name="" package="SC74_INFINEON">
<connects>
<connect gate="G$1" pin="EN/PWM" pad="3"/>
<connect gate="G$1" pin="GND" pad="2 5"/>
<connect gate="G$1" pin="VDRIVE" pad="4"/>
<connect gate="G$1" pin="VS" pad="1"/>
<connect gate="G$1" pin="VSENSE" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLE5009" prefix="IC">
<description>&lt;b&gt;GMR-Based (Giant Magneto Resistance)  Angular Sensor&lt;/b&gt;&lt;p&gt;
Source: Infineon, TLE5009_FDS_Rev.1.1.pdf</description>
<gates>
<gate name="G$1" symbol="TLE5009"/>
</gates>
<devices>
<device name="" package="PG-DSO-8">
<connects>
<connect gate="G$1" pin="COS_N" pad="2"/>
<connect gate="G$1" pin="COS_P" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="SIN_N" pad="7"/>
<connect gate="G$1" pin="SIN_P" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VGMR" pad="5"/>
</connects>
<technologies>
<technology name="-E1000"/>
<technology name="-E1010"/>
<technology name="-E2000"/>
<technology name="-E2010"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IPB180N06S4-H1" prefix="IC">
<description>&lt;b&gt;OptiMOS®-T2 Power-Transistor&lt;/b&gt;&lt;p&gt;
Source: 1859075.pdf (Farnell)</description>
<gates>
<gate name="G$1" symbol="NMOS-FET-E"/>
</gates>
<devices>
<device name="" package="PG-TO263-7-3">
<connects>
<connect gate="G$1" pin="D" pad="8"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2 3 5 6 7" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF7580">
<gates>
<gate name="G$1" symbol="IRF7580"/>
</gates>
<devices>
<device name="" package="DIRECT-FET-ME">
<connects>
<connect gate="G$1" pin="D" pad="D@1 D@2"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S@1 S@2 S@3 S@4 S@5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF7480" prefix="U">
<gates>
<gate name="G$1" symbol="IRF7480"/>
</gates>
<devices>
<device name="" package="DIRECT-FET-ME">
<connects>
<connect gate="G$1" pin="D" pad="D@1 D@2"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S@1 S@2 S@3 S@4 S@5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRLHS2242" prefix="Q">
<gates>
<gate name="G$1" symbol="IRLHS2242TR"/>
</gates>
<devices>
<device name="" package="PQFN">
<connects>
<connect gate="G$1" pin="D" pad="D@1 D@2 D@3 D@4 D@5"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S@1 S@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
