<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<packages>
<package name="BC832">
</package>
</packages>
<symbols>
<symbol name="BC832">
<description>Fanstel's castellated package BC832 chip</description>
<pin name="GND"/>
<pin name="P20"/>
<pin name="SWDIO"/>
<pin name="SWCLK"/>
<pin name="P18"/>
<pin name="P13"/>
<pin name="P11/TX"/>
<pin name="P12/RX"/>
<pin name="P03/AIN1"/>
<pin name="P21/RESET"/>
<pin name="P00/XL1"/>
<pin name="P01/XL2"/>
<pin name="P02/AIN0"/>
<pin name="P27/SCL"/>
<pin name="P26/SDA"/>
<pin name="VDD"/>
<pin name="A1/P28"/>
<pin name="A2/P17"/>
<pin name="A3/P04"/>
<pin name="A4/P06"/>
<pin name="A5/P08"/>
<pin name="B1/P25"/>
<pin name="B2/P29"/>
<pin name="B3/P31"/>
<pin name="B4/P05"/>
<pin name="B5/P07"/>
<pin name="C1/P24"/>
<pin name="C2/P22"/>
<pin name="C3/P30"/>
<pin name="C4/P15"/>
<pin name="C5/P09"/>
<pin name="D1/P23"/>
<pin name="D2/P19"/>
<pin name="D3/P16"/>
<pin name="D4/P14"/>
<pin name="D5/P10"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BC832" prefix="U">
<gates>
<gate name="G$1" symbol="BC832"/>
</gates>
<devices>
<device name="" package="BC832">
<connects>
<connect gate="G$1" pin="A1/P28" pad="P$A1"/>
<connect gate="G$1" pin="A2/P17" pad="P$A2"/>
<connect gate="G$1" pin="A3/P04" pad="P$A3"/>
<connect gate="G$1" pin="A4/P06" pad="P$A4"/>
<connect gate="G$1" pin="A5/P08" pad="P$A5"/>
<connect gate="G$1" pin="B1/P25" pad="P$B1"/>
<connect gate="G$1" pin="B2/P29" pad="P$B2"/>
<connect gate="G$1" pin="B3/P31" pad="P$B3"/>
<connect gate="G$1" pin="B4/P05" pad="P$B4"/>
<connect gate="G$1" pin="B5/P07" pad="P$B5"/>
<connect gate="G$1" pin="C1/P24" pad="P$C1"/>
<connect gate="G$1" pin="C2/P22" pad="P$C2"/>
<connect gate="G$1" pin="C3/P30" pad="P$C3"/>
<connect gate="G$1" pin="C4/P15" pad="P$C4"/>
<connect gate="G$1" pin="C5/P09" pad="P$C5"/>
<connect gate="G$1" pin="D1/P23" pad="P$D1"/>
<connect gate="G$1" pin="D2/P19" pad="P$D2"/>
<connect gate="G$1" pin="D3/P16" pad="P$D3"/>
<connect gate="G$1" pin="D4/P14" pad="P$D4"/>
<connect gate="G$1" pin="D5/P10" pad="P$D5"/>
<connect gate="G$1" pin="GND" pad="P$1"/>
<connect gate="G$1" pin="P00/XL1" pad="P$11"/>
<connect gate="G$1" pin="P01/XL2" pad="P$12"/>
<connect gate="G$1" pin="P02/AIN0" pad="P$13"/>
<connect gate="G$1" pin="P03/AIN1" pad="P$9"/>
<connect gate="G$1" pin="P11/TX" pad="P$7"/>
<connect gate="G$1" pin="P12/RX" pad="P$8"/>
<connect gate="G$1" pin="P13" pad="P$6"/>
<connect gate="G$1" pin="P18" pad="P$5"/>
<connect gate="G$1" pin="P20" pad="P$2"/>
<connect gate="G$1" pin="P21/RESET" pad="P$10"/>
<connect gate="G$1" pin="P26/SDA" pad="P$15"/>
<connect gate="G$1" pin="P27/SCL" pad="P$14"/>
<connect gate="G$1" pin="SWCLK" pad="P$4"/>
<connect gate="G$1" pin="SWDIO" pad="P$3"/>
<connect gate="G$1" pin="VDD" pad="P$16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
